Average annual load and average percent change relative to FWO (NA25) over the simulation period or record between May 1965 and April 2016 for back flow/pumping from S77, S308 and EAA (S2, S3 and S4) to Lake Okeechobee.

|  | | Average Annual1 | | | | % Change Compare to FWO | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Area | Alt1 | Percent Total Inflow Water Budget1 | Discharge (kAcf-Ft WY⁻¹)1 | TP Load (kg WY⁻¹) | TN Load (kg WY⁻¹) | Discharge | TP Load | TN Load |
| S77 | NA25 | 1.8% | 34.0 | 5957 | 70334 | --- | --- | --- |
| ECBr | 1.8% | 35.2 | 6370 | 74002 | 3.7 | 6.9 | 5.2 |
| CC | 1.6% | 31.5 | 5839 | 66730 | -7.3 | -2.0 | -5.1 |
| S308 | NA25 | 2.1% | 38.8 | 9894 | 84024 | --- | --- | --- |
| ECBr | 2.4% | 45.9 | 11421 | 96162 | 18.2 | 15.4 | 14.4 |
| CC | 2.4% | 45.6 | 11882 | 101066 | 17.5 | 20.1 | 20.3 |
| EAA | NA25 | 2.5% | 47.3 | 13790 | 169512 | --- | --- | --- |
| ECBr | 2.7% | 52.8 | 14516 | 187490 | 11.7 | 5.3 | 10.6 |
| CC | 3.4% | 64.4 | 15760 | 228985 | 36.2 | 14.3 | 35.1 |
| 1Simulation period of record between Florida Water Year 1966 - 2016 (May 1965 - April 2016) | | | | | | | | |